{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Tabelle1","Tabelle2","Tabelle3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Tabelle1","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
[null,null,null,"Nutzlastmassen des Experimental-Ballons Xploer25"]
[]
[]
[]
[null,null,"Baugruppe","Masse[g]","Bemerkung"]
[]
[null,null,"LiPO-Akkupack mit Stecker",48]
[null,null,"RaspberryPI (original)",39]
[null,null,"RaspberryPI mit Siftleiste-Stecker entfernt",24,"nur P1,S2,S3,S5"]
[null,null,"Kamera für RaspberryPI"]
[null,null,"HF-Platine komplett ohne Antennen"]
[null,null,"Antennen"]
[null,null,"GPS-Platine",30,"mit Metallgehäuse ohne Kabel"]
[null,null,"Kleinteile"]
[null,null,"Nutzlast unverkleidet"]
[null,null,"Nutzlast verkleidet"]
[null,null,"Abtrenneinheit"]
[null,null,"Nutzlast + Abtrenneinheit"]
[null,null,"Nutzlast+Abtrenneinheit+Fallschirm"]
[null,null,"Nutzlast+Abtrenneinheit+Fallschirm+Ballonhülle"]
[]
[{"$nulls":4},"Stand 10. Januar 2014 DL2ARH"]

{"sheet":"Tabelle2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Tabelle3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}